From 1bc5aee63eb72b341f506ad058502cd0361f0d10 Mon Sep 17 00:00:00 2001
From: Ben Cheng <bccheng@google.com>
Date: Tue, 25 Mar 2014 22:37:19 -0700
Subject: Initial checkin of GCC 4.9.0 from trunk (r208799).

Change-Id: I48a3c08bb98542aa215912a75f03c0890e497dba
---
 gcc-4.9/gcc/config/sh/sh-modes.def | 34 ++++++++++++++++++++++++++++++++++
 1 file changed, 34 insertions(+)
 create mode 100644 gcc-4.9/gcc/config/sh/sh-modes.def

(limited to 'gcc-4.9/gcc/config/sh/sh-modes.def')

diff --git a/gcc-4.9/gcc/config/sh/sh-modes.def b/gcc-4.9/gcc/config/sh/sh-modes.def
new file mode 100644
index 0000000..3aa3046
--- /dev/null
+++ b/gcc-4.9/gcc/config/sh/sh-modes.def
@@ -0,0 +1,34 @@
+/* SH extra machine modes. 
+   Copyright (C) 2003-2014 Free Software Foundation, Inc.
+
+This file is part of GCC.
+
+GCC is free software; you can redistribute it and/or modify
+it under the terms of the GNU General Public License as published by
+the Free Software Foundation; either version 3, or (at your option)
+any later version.
+
+GCC is distributed in the hope that it will be useful,
+but WITHOUT ANY WARRANTY; without even the implied warranty of
+MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+GNU General Public License for more details.
+
+You should have received a copy of the GNU General Public License
+along with GCC; see the file COPYING3.  If not see
+<http://www.gnu.org/licenses/>.  */
+
+/* The SH uses a partial integer mode to represent the FPSCR register.  */
+PARTIAL_INT_MODE (SI, 22, PSI);
+/* PDI mode is used to represent a function address in a target register.  */
+PARTIAL_INT_MODE (DI, 64, PDI);
+
+/* Vector modes.  */
+VECTOR_MODE  (INT, QI, 2);    /*                 V2QI */
+VECTOR_MODES (INT, 4);        /*            V4QI V2HI */
+VECTOR_MODES (INT, 8);        /*       V8QI V4HI V2SI */
+VECTOR_MODES (INT, 16);       /* V16QI V8HI V4SI V2DI */
+VECTOR_MODES (FLOAT, 8);      /*            V4HF V2SF */
+VECTOR_MODES (FLOAT, 16);     /*       V8HF V4SF V2DF */
+VECTOR_MODE (INT, DI, 4);     /*                 V4DI */
+VECTOR_MODE (INT, DI, 8);     /*                 V8DI */
+VECTOR_MODE (FLOAT, SF, 16);  /*                V16SF */
-- 
cgit v1.1

